{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["List 1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"List 1","index":0,"n_rows":14,"n_cols":8,"rows_kept":14,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,"Kód","Název","Semestr","Rozsah, examinace","Katedra","Fakulta","4EU+"]
[null,"M148005","Laboratoř technologie konzervování-restaurování","zimní","zimní s.:0/10, KZ [HT]",148,"FCHT","ne"]
[null,"B106015","Koroze a degradace kovů","zimní","zimní s.:2/0, Zk [HT]",106,"FCHT","ne"]
[null,"P106006","Mechanismy degradace kovových materiálů a metody jejich konzervace","zimní","zimní s.:3/0, Jiné [HT]",106,"FCHT","ne"]
[null,"B148002","Anorganické materiály památek II","zimní","zimní s.:3/0, Zk [HT]",148,"FCHT","ne"]
[null,"B148033","Laboratoř programu konzervování-restaurování","zimní","zimní s.:0/5, KZ [HT]",148,"FCHT","ne"]
[null,"M150002","Laboratorní projekt chemie a technologie materiálů I","letní","letní s.:0/10, KZ [HT]",126,"FCHT","ne"]
[null,"M150003","Laboratorní projekt chemie a technologie materiálů II","zimní","zimní s.:0/12, KZ [HT]",106,"FCHT","ne"]
[null,"AB106002","Materials Corrosion","zimní","zimní s.:3/0, Zk [HT]",106,"FCHT","ne"]
[null,"B106002","Koroze materiálů","zimní","zimní s.:3/0, Zk [HT]",106,"FCHT","ne"]
[null,"B148046","Semestrální projekt studijního programu","zimní","zimní s.:0/10, KZ [HT]",148,"FCHT","ne"]
[null,"B148044","Seminář k bakalářské práci programu technologie konzervování-restaurování","letní","letní s.:0/2, Z [HT]",148,"FCHT","ne"]
[null,"P106001","Teorie korozních procesů","oba"," 3/0, Jiné [HT]",106,"FCHT","ne"]
[null,"AP106001","Theory of Corrosion Processes","oba"," 3/0, Jiné [HT]",106,"FCHT","ne"]