{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["List 1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"List 1","index":0,"n_rows":12,"n_cols":8,"rows_kept":12,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,"Kód","Název","Semestr","Rozsah, examinace","Katedra","Fakulta","4EU+"]
[null,"N409004","Chemicko-inženýrský projekt","oba"," 0/1, KZ [HT]",409,"FCHI","ne"]
[null,"B409001","Chemické inženýrství I","oba"," 2/3, Z+Zk [HT]",409,"FCHI","ne"]
[null,"N409003","Chemické inženýrství II","oba"," 2/3, Z+Zk [HT]",409,"FCHI","ne"]
[null,"AM409003","Process and System Engineering","letní","letní s.:2/2, Z+Zk [HT]",409,"FCHI","ne"]
[null,"M409064","Modelování proudění metodou CFD","letní","letní s.:0/20, KZ [HS]",599,"FCHI","ne"]
[null,"N409004A","Chemicko-inženýrský projekt","letní","letní s.:0/1, KZ [HT]",409,"FCHI","ne"]
[null,"M413006","Metody analýzy nelineárních dynamických modelů","letní","letní s.:2/2, Z+Zk [HT]",413,"FCHI","ne"]
[null,"M409003","Procesní a systémové inženýrství","letní","letní s.:2/2, Z+Zk [HT]",409,"FCHI","ne"]
[null,"M409012","Procesní inženýrství a design","zimní","zimní s.:1/2, Z+Zk [HT]",409,"FCHI","ne"]
[null,"AM409012","Process Engineering and Design","zimní","zimní s.:1/2, Z+Zk [HT]",409,"FCHI","ne"]
[null,"N409060","Procesní inženýrství a design","zimní","zimní s.:1/2, Z+Zk [HT]",409,"FCHI","ne"]